[bookmark: _Hlk481127608]LEED for Neighborhood Development Power Jam Study
Quiz #3 – Neighborhood Pattern and Design (NPD))

1. NPD Prerequisite Connected and Open Community, Case 2 Internal Connectivity requires projects to design and build the project such that its internal connectivity is at least
A. [bookmark: _GoBack]140 intersections per square mile
B. 90 intersections per square mile
C. 1 intersection every 800 feet
D. 1 intersection every 500 feet

2. To meet walkable streets, new residential-only motorized parts of the circulation network within the project should be designed for a target speed of no more than
A. 15 mph
B. 20 mph
C. 25 mph
D. 30 mph

3. Which of these is used to calculate the probability that any two randomly selected dwelling units in a project will be of a different type?
A. Area Median Income (AMI)
B. Housing and Urban Development (HUD)
C. Simpson Diversity Index
D. Qualified Census Tract (QCT)

4. A project design team was asked by the owner to replace a black asphalt parking lot with grey pervious concrete in order to achieve Rainwater Management. What other environmental impact is reduced by this design change?
A. Emissivity
B. Heat island effect
C. Light Pollution
D. Daylight
5. Which of these may be prohibited in front yards that face the circulation network?
A. Gardens
B. Raised vegetable beds
C. Pots for growing herbs
D. Greenhouses
6. Determine the minimum number of trees required for Neighborhood Pattern and Design Credit Tree-Lined and Shaded Streetscapes, Option 1. Tree-Lined Blocks if the total existing and planned block length within the project is 3500 lf.
A. 30
B. 35
C. 42
D. 70
7. Which of these would meet the requirement for New school campuses within the project boundary for earning the Neighborhood Pattern and Design (NPD) Credit Neighborhood Schools?
A. Elementary School to be built on 4 acres
B. High School to be built on 20 acres
C. Middle School to be built on 15 acres
D. Combined Middle and High School to be built on 35 acres
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