|  |  |
| --- | --- |
| A green square with white text  Description automatically generated | **Green Building Practices and LEED Green Associate Exam Preparation** |

**Lorisweb.com**

**GA02 Introductory and Overview Sections. LEED Building Design +Construction Reference Guide. v4 Edition**

**Reference Guide Overview**

**A screenshot of a computer screen

Description automatically generated**

**Getting Started**

How to Use this Reference Guide

**Credit Categories**

A group of black circles with white text

Description automatically generated

A close-up of a document

Description automatically generated

**Projects Outside the US**

**International Tips**

This section offers advice on how to determine equivalency to U.S. Standards or using non-U.S. standards referenced in the rating system.

**Inch-Pound (IP)** - inch, pound, and gallon

Derived from the English system and commonly used in the U.S.

**International System of Units (SI)** – meter, kilogram, and liter

Metric system used in most other parts of the world and defined by the General Conference on Weights and Measures.

**“local equivalent”**

* Means an alternative to a LEED referenced standard that is specific to a project’s locality. “Whichever is more stringent”

**“USGBC-approved local equivalent”**

* Means a local standard deemed equivalent to the listed standard by the U.S. Green Building Council through its process for establishing non-U.S. equivalencies in LEED.

**Example - SS Prerequisite Construction Activity Pollution Prevention**

A close-up of a document

Description automatically generated

**Taking an Integrative Approach to Design and Construction**

A diagram of elements of integrated design

Description automatically generated

**Integrative Design Process**

* Engage all project team members.
* Work in collaboration not isolation.
* Look for interrelationships and synergies between systems and components.

The coordination of building and site systems should be addressed early, preferably **before schematic design**.

The **Integrative Process credit** formally introduces this way of working into LEED so that the team members’ expertise in building and site systems can inform the performance, efficiency, and effectiveness of every system.

“When areas of practice are integrated, it becomes possible to significantly improve building performance and achieve synergies that yield economic, environmental, and human health benefits.”

A diagram of a diagram

Description automatically generated

**Integrative Process Includes Three Phases:**

**Discovery.** The most important phase of the integrative process, discovery can be thought of as an extensive expansion of what is conventionally called predesign. A project is unlikely to meets its environmental goals cost-effectively without this discrete phase. Discovery work should take place before schematic design begins.

**Design and construction (implementation).** This phase begins with what is conventionally called schematic design. It resembles conventional practice but integrates all the work and collective understanding of system interactions reached during the discovery phase.

**Occupancy, operations, and performance feedback.** This third stage focuses on preparing to measure performance and creating feedback mechanisms. Assessing performance against targets is critical for informing building operations and identifying the need for any corrective action.

**The structure to manage this flow of people, information, and analysis is as follows:**

* All project team members, representing all design and construction disciplines, gather information and data relevant to the project.
* Team members analyze their information.
* Team members participate in **workshops** to compare notes and identify opportunities for synergy.

This process of research, analysis, and workshops is done in an iterative cycle that refines the design solutions.

**Devising a LEED Work Plan**

A diagram of a program

Description automatically generated with medium confidence

**Maintaining Consistency in the LEED Application**

Certain issues recur across multiple credits and credit categories and must be treated consistently throughout the submission.

**Special Project Situations**

Projects with a combination of space types or unusual space types should pay particular attention to how these characteristics influence credit achievement.

**Common project programs that require additional consideration include the following:**

* Mixed Use
* Multitenant Complex
* Incomplete Spaces
* Projects with Several Physically Distinct Structures

**Mixed Use**

Examples

**Residential and Commercial**

A multi-family residential building with 8 occupiable stories above grade certifying under BD+C: New Construction includes a retail grocery store on the ground level, the team could benefit from guidance for BD+C: Retail projects.

**Commercial and Data Center**

An office building certifying under BD+C: New Construction includes a small data center, the team should follow the data center guidelines for certain credits; these guidelines are not limited to BD+C: Data Centers projects.

**Hospitality and Retail**

A hotel project certifying under BD+C: Hospitality; in designing the retail spaces on the hotel’s ground floor, the team could benefit from guidance for BD+C: Retail projects.

**Multitenant Complex**

* Some projects may be part of a large complex of buildings or a master planned development.
* Any project can follow the multitenant complex approach if it is part of a master plan development, regardless of whether the project is using the LEED Campus approach.

**Incomplete Spaces**

* No more than 40% of the certifying gross floor area of a LEED project may consist of incomplete space unless the project is using the LEED BD+C: Core and Shell rating system.
* Projects that include incomplete spaces must use [Appendix 2](file:///D:\Dropbox\03%20My%20Life\Fall%202019\03%20CMGT380%20Fall%202019\01%20Reading%20Material\GA02%20Excerpt_v4_BDC-12%20Appendix%202.pdf) Default Occupancy Counts to establish occupant counts for incomplete spaces.
* For incomplete spaces in projects using a rating system other than LEED BD+C: Core and Shell, the project team must provide supplemental documentation.
  + Submit a letter of commitment, signed by the owner.
  + Incomplete spaces intended to be finished by tenants (i.e., parties other than the owner), submit a set of nonbinding tenant design and construction guidelines.

**Projects with Several Physically Distinct Structures**

Primary and secondary school projects, hospitals (general medical and surgical), hotels, resorts, and resort properties, as defined for ENERGY STAR building rating purposes, are eligible to include more than one physically distinct structure in a single LEED project certification application without having to use the Campus Program, subject to the following conditions.

* The buildings to be certified must be a part of the same identity. For example, the buildings are all part of the same elementary school, not a mix of elementary school and high school buildings.
* The project must be analyzed as a whole (i.e., in aggregate) for all minimum program requirements (MPRs), prerequisites, and credits in the LEED rating system.
* All the land area and all building floor areas within the LEED project boundary must be included in every prerequisite and credit submitted for certification.
* There is no specific limit on the number of structures, but the aggregate gross floor area included in a single project must not exceed 1 million square feet (92,905 square meters).
* Any single structure that is larger than 25,000 square feet (2,320 square meters) must be registered as a separate project or treated as a separate building in a group certification approach.

**Renovations and Additions**

Refer to the [minimum program requirements](file:///D:\Dropbox\03%20My%20Life\Fall%202019\03%20CMGT380%20Fall%202019\01%20Reading%20Material\GA02%20Excerpt_v4_BDC-2%20MPRs.pdf) for information on how boundaries should be drawn for renovation and addition projects.

Additionally, use the following guidance for treating energy systems in any project with mechanical systems.

**Separate systems**. Mechanical systems are completely separate from those in the existing building (emergency generators excepted) and can be modeled separately.

**Shared central systems located outside the project building or space**. Each prerequisite and credit section related to energy modeling offers specific guidance on how to handle this situation; in particular, see the guidance for EA Prerequisite Minimum Energy Performance.

**Tenant Sales and Lease Agreement**

LEED BD+C: Core and Shell

Credits or thresholds beyond the construction scope of the LEED project, a binding tenant sales and lease agreement must be provided as documentation.

This must be signed by the future tenant and include terms related to how the technical credit requirements will be carried out by the tenant.

**Previous Development**

**previously developed** altered by paving, construction, and/or land use that would typically have required regulatory permitting to have been initiated (alterations may exist now or in the past). Land that is not previously developed and landscapes altered by current or historical clearing or filling, agricultural or forestry use, or preserved natural area use are considered undeveloped land. The date of previous development permit issuance constitutes the date of previous development, but permit issuance in itself does not constitute previous development.

**previously developed site** a site that, prior to the project, consisted of at least 75% previously developed land.

**previously disturbed** areas that have been graded, compacted, cleared, previously developed, or disturbed in any way. These are areas that do not qualify as 'greenfield.’

**LEED Sites**

**Greenfield** - area that has not been graded, compacted, cleared, or disturbed and that supports (or could support) open space, habitat, or natural hydrology.

**Brownfield** - real property or the expansion, redevelopment, or reuse of which may be complicated by the presence or possible presence of a hazardous substance, pollutant, or contaminant.

**Hardscape** - the inanimate elements of the building landscaping. It includes pavement, roadways, stonewalls, wood and synthetic decking, concrete paths and sidewalks, and concrete, brick, and tile patios.

**Buildable Land** - the portion of the site where construction can occur, including land voluntarily set aside and not constructed on. When used in density calculations, buildable land excludes public rights-of-way and land excluded from development by codified law.

LEED ND: the portion of the site where construction can occur, including land voluntarily set aside and not constructed on. When used in density calculations, buildable land excludes public rights-of-way and land excluded from development by codified law or LEED for Neighborhood Development prerequisites.

**Development Footprint**

A project’s development footprint is all of its impervious surfaces.

**development footprint** the total land area of a project site covered by buildings, streets, parking areas, and other typically impermeable surfaces constructed as part of the project.

Surfaces paved with permeable pavement (at least 50% permeable) are excluded from the development footprint.

A close-up of a brick walkway

Description automatically generated

A diagram of a house and a street

Description automatically generated with medium confidence**Density**

A measure of the total building floor area or dwelling units on a parcel of land relative to the buildable land of that parcel. Units for measuring density may differ according to credit requirements. Does not include structured parking.

**Floor-Area Ratio (FAR)**

The density of nonresidential land use, exclusive of parking, measured as the total nonresidential building floor area divided by the total buildable land area available for nonresidential structures.

A diagram of a building structure

Description automatically generated

A diagram of a building

Description automatically generated

A diagram of a building

Description automatically generated

**Determine the FAR**

A LEED for Retail project has a total floor area of 12,400 square feet and the total buildable land is 0.4 hectacre. What is the Floor-Area Ratio for the project?

**Occupancy**

Regular Building Occupants Visitors

Part-time and full-time employees Retail customers

Staff Outpatients

Volunteers – regularly use a building Volunteers – periodically use a building

Residents Higher-education students

Primary and secondary school students

Hotel guests

Inpatients

A screenshot of a computer

Description automatically generated

A black and white text

Description automatically generated

**In calculations, occupant types are typically counted in two ways:**

**Daily averages** take into account all the occupants of a given type for a typical 24-hour day of operation.

**Peak totals** are measured at the moment in a typical 24-hour period when the highest number of a given occupant type is present.

**Whenever possible, use actual or predicted occupancies.**

**If occupancy cannot be accurately predicted, use one of the following resources to estimate occupancy:**

* Default occupant density from ASHRAE 62.1-2010, Table 6-1
* Default occupant density from CEN Standard EN 15251, Table B.2
* Appendix 2 Default Occupancy Counts
* Results from applicable studies.

If numbers vary seasonally, use occupancy numbers that are a representative daily average over the entire operating season of the building.

If occupancy patterns are atypical (shift overlap, significant seasonal variation), explain such patterns when submitting documentation for certification.

Example

1. A LEED project has 8 employees that work 4 hours per day, 12 employees that work 6 hours per day and 20 employees that work 8 hours per day. What is the total Full Time Equivalent (FTE) for the project?
2. 37
3. 33
4. 35
5. 38

**Minimum Program Requirements (MPRs)**

The Minimum Program Requirements (MPRs) are the minimum characteristics or conditions that make a project appropriate to pursue LEED certification. These requirements are foundational to all LEED projects and define the types of buildings, spaces, and neighborhoods that the LEED rating system is designed to evaluate.

Purpose:

1. Give clear guidance to customers
2. Protect the integrity of the LEED program
3. Reduce challenges that occur during the LEED certification process

1. **Must be in a permanent location on existing land**

Requirements

* All LEED projects must be constructed and operated on a permanent location on existing land.
* No project that is designed to move at any point in its lifetime may pursue LEED certification.
* This requirement applies to all land within the LEED project.

2. **Must use reasonable LEED boundaries**

Requirements

* The LEED project boundary must include all contiguous land that is associated with the project and supports its typical operations.
* The LEED boundary may not unreasonably exclude portions of the building, space, or site to give the project an advantage in complying with credit requirements.
* The LEED project must accurately communicate the scope of the certifying project in all promotional and descriptive materials and distinguish it from any non-certifying space.

3. **Must comply with project size requirements**

Requirements

* LEED BD+C: minimum 1,000 square feet of gross floor area
* LEED O+M: minimum 1,000 square feet of gross floor area
* LEED ID+C: minimum 250 square feet of gross floor area
* LEED for Homes: defined as a “dwelling unit” by all applicable codes
* LEED for ND: at least 2 habitable buildings, no larger than 1500 acres

**Rating System Selection Guidance**

Before Registering a project:

1. Identify an appropriate rating system
2. Determine the best adaptation

If a project team selects a rating system that doesn't apply, USGBC may request that they change the project's rating system.

**Minimum Program Requirements (MPRs)**

The first step should be to make sure that LEED will work for your project no matter what rating system is selected.

Verify project can satisfy all of the LEED v4 Minimum Program Requirements.

Contact USGBC if it is not clear which rating system should be used.

**Examples**

An owner wants to LEED certify an existing office building and commit to on-going sustainability goals. Which rating system would you recommend?

1. LEED for Interior Design and Construction
2. LEED for Building Design and Construction
3. LEED for Building Operations and Maintenance
4. LEED for Neighborhood Development

A new tenant in a commercial office building wants to pursue LEED certification. Which rating system would you recommend they use?

1. LEED for Interior Design and Construction
2. LEED for Building Design and Construction
3. LEED for Building Operations and Maintenance
4. LEED for Neighborhood Development

What LEED rating system focuses on the where, what, and how to build green at a community scale?

1. LEED BD+C: Retail
2. LEED BD+C: Schools
3. LEED BD+C: New Construction
4. LEED for Neighborhood Development

**Choosing Between Rating Systems**





