LEED for Neighborhood Development
Activity #2
Before completing this Activity Read: Reference Guide for Neighborhood Development v4 – Pages 59-168

[bookmark: _GoBack]Fill-In, Multiple Choice, Matching
Although the LEED ND reference guide does not number the LEED prerequisites and credits, for this exercise they have been numbered in the order presented in the credit category.

1. Test your knowledge of how well you know the names of the credits for the Smart Location and Linkage (SLL) credit category:
	Credit
	Name

	P1
	

	P2
	

	P3
	

	P4
	

	P5
	

	C1
	

	C2
	

	C3
	

	C4
	

	C5
	

	C6
	

	C7
	

	C8
	

	C9
	



2. Match the intent shown below to the prerequisite or credit:
	Credit
	ANS
	
	Credit
	ANS

	SLL – P1
	
	
	SLL – C3
	

	SLL – P2
	
	
	SLL – C4
	

	SLL – P3
	
	
	SLL – C5
	

	SLL – P4
	
	
	SLL – C6
	

	SLL – P5
	
	
	SLL – C7
	

	SLL – C1
	
	
	SLL – C8
	

	SLL – C2
	
	
	SLL – C9
	











	
	INTENT

	A
	To encourage development within existing cities, suburbs, and towns to reduce the environmental and public health consequences of sprawl. To reduce development pressure beyond the limits of existing development. To conserve the natural and financial resources required for infrastructure.

	B
	To conserve imperiled species and ecological communities.

	C
	To encourage balanced communities with a proximate housing and employment opportunities.

	D
	To encourage the cleanup of contaminated lands and developing sites that have been identified as contaminated.

	E
	To preserve irreplaceable agricultural resources by protecting prime and unique farmland from development.

	F
	To restore native plants, wildlife habitat, wetlands, and water bodies harmed by previous human activities.

	G
	To protect life and property, promote open space and habitat conservation, and enhance water quality and natural hydrologic systems.

	H
	To encourage development within and near existing communities and public transit infrastructure. To encourage improvement and redevelopment of existing cities, suburbs, and towns while limiting the expansion of the development footprint in the region. To reduce vehicle trips and vehicle distance traveled. To reduce the incidence of obesity, heart disease, and hypertension by encouraging daily physical activity associated with walking and bicycling.

	I
	To promote bicycling and transportation efficiency and reduce vehicle distance traveled. To improve public health by encouraging utilitarian and recreational physical activity.

	J
	To minimize erosion, protect habitat, and reduce stress on natural water systems by preserving steep slopes in a natural, vegetated state.

	K
	To preserve water quality, natural hydrology, habitat, and biodiversity through conservation of wetlands and water bodies.

	L
	To conserve native plants, wildlife habitat, wetlands, and water bodies.

	M
	To encourage development in locations shown to have multimodal transportation choices or otherwise reduced motor vehicle use, thereby reducing greenhouse gas emissions, air pollution, and other environmental and public health harms associated with motor vehicle use.



3. Smart Location and Linkage focuses on selection of sites that minimize the adverse environmental effects of new development and avoid contributing to ________________ and its consequences.

4. Increased automobile travel is one of the most damaging consequences of ________________.

5. In addition, the ________________and ________________ surfaces required to support vehicular travel consume land and nonrenewable resources, disrupt ________________ rainwater flow, and enlarge urban ________________________________.

6. To reduce the effects of sprawl and create more livable communities, preference should be given to locations _______________ to existing town and city centers, sites with good _______________ access, _______________ sites, _______________ developed sites, and sites _______________ to existing development.

7. Selection of sites that are within or adjacent to _______________ development can minimize habitat ____________________________ and also help preserve areas for recreation.

8. ______________________ patterns of development not only take these lands out of agricultural production but can also ___________________ farming communities and consequently reduce the ________________ viability of the local agricultural economy.

9. SSL Prerequisite: Smart Location
Requirements
For All Projects
Either (1) locate the project on a site served by _______________ water and wastewater infrastructure or (2) locate the project within a legally _______________, publicly owned, planned water and wastewater service area, and provide new water and wastewater infrastructure for the project.

The site should also meet the requirements of one of the following four options.

OPTION 1. __________________________________
Locate the project on an _______________ site.

OR
OPTION 2. ______________________________________________
Locate the project on an _______________ site (i.e., a site that is adjacent to _______________ developed land) where the connectivity of the adjacent land is at least ________ intersections per square mile as measured within a ________-mile distance of a continuous segment of the project boundary that constitutes at least ________ of the total project boundary and is adjacent to previous development.
Existing intersections may be counted if they were not constructed or funded by the project developer within the past ________ years.

Locate and/or design the project such that a through-connection (of the circulation network) intersects the adjacent portion of the project boundary at least every ________ feet on average and at least every ________ feet, connecting it with an existing circulation network outside the project; nonmotorized through-connections of the circulation network may count for no more than ________ of the total. The exemptions listed in NPD Prerequisite Connected and Open Community do not apply to this option.

OR
OPTION 3. _____________________________
Locate the project on a site with existing or planned transit service such that at least ________ of dwelling units and nonresidential use entrances (inclusive of existing buildings) are within a ________-mile walking distance of at least ________ bus, streetcar, or rideshare stop, or within a ________-mile walking distance of at least ________ bus rapid transit stop, light or heavy rail station, or commuter ferry terminal. The transit service at the stop(s) in aggregate must meet the minimums listed in Table 1.

Projects must meet the requirements for __________ weekday and weekend trips and provide service ____________ day.

	TABLE 1. Minimum daily transit service

	
	Weekdays
	Weekends

	Projects with multiple transit types (bus, streetcar, rail, or ferry)
	
	

	Projects with commuter rail or ferry service only
	
	



If transit service is _______________ but not yet operational, the project must demonstrate one of the following:
1. The relevant transit agency has a _______________ full-funding grant agreement with the Federal Transit Administration (or equivalent national agency for project outside the U.S.) that includes a revenue operations date for the start of transit service. The revenue operations date must be no later than the date by which ________ of the project’s total building _______________ floor area will be occupied.

2. For bus, streetcar, bus rapid transit, or ferry service, the transit _______________ must certify that it has an approved _______________ that includes specifically allocated funds sufficient to provide the planned service at the levels listed above and that service at these levels will begin no later than the date by which ________ of the project’s total building _______________ floor area will be occupied.

3. For rail service other than streetcars, the transit agency must certify that __________________ engineering for a rail line has begun. In addition, the service must meet either of these two requirements:
· A state legislature or local subdivision of the state (or a local government for projects outside the U.S.) has authorized the transit agency to expend funds to establish rail transit service that will begin no later than the date by which ________ of the project’s total building _______________ floor area will be occupied.
OR
· A local government has dedicated funding or reimbursement commitments from future tax revenue for the development of stations, platforms, or other rail transit infrastructure that will serve the project no later than the date by which ________ of the project’s total building _______________ floor area will be occupied.

OR
OPTION 4. _______________________________________________________________
Include a residential component equaling at least ________ of the project’s total building gross floor area (exclusive of portions of _______________ structures devoted exclusively to parking) and locate the project near _______________ uses (see Appendix 1) such that the project boundary is within a ________ -mile walking distance of at least ________ uses, or such that the project’s geographic center is within a    ________ -mile walking distance of at least ________ uses.

The following restrictions apply.
A ________ counts as only ________ type (e.g., a retail store may be counted only once even if it sells products in several categories).
No more than ________ uses in each use ________ may be counted (e.g., if five restaurants are within the required distance, only ________ may be counted).
The uses accessible to the project must represent at least ________ categories.

Four types of project locations meet the requirements of SSL Prerequisite Smart Location:
_______________ sites
sites that are _______________ to well-connected parcels of land
sites served by _______________ , and
sites near a variety of _______________________ uses.

Each type helps limit ________________, promote alternative ___________________________, modes, reduce vehicle ________________, traveled, and ________________, neighborhoods.

Infrastructure must be ________________ owned. ________________ and mound wastewater treatment systems _______________ qualify.

10. SS Prerequisite: Imperiled Species and Ecological Communities Conservation
Requirements
Consult with the state Natural Heritage Program and state fish and wildlife agencies (or local equivalent for projects outside the U.S.) to determine if any of the following have been or are likely to be found on the project site because of the presence of suitable habitat and nearby occurrences:
species listed as threatened or endangered under the U.S. _________________________ Species Act or the state’s _________________________ species act, or
species or ecological communities classified by _________________________  as ________ (possibly extinct), ________ (critically imperiled), or ________ (imperiled), or
species listed as threatened or endangered specified under ________________ equivalent standards (in areas outside the U.S.) that are not covered by NatureServe data.

If the consultations are inconclusive and site conditions indicate that imperiled species or ecological communities could be present, perform _________________________ surveys using accepted methodologies during appropriate _________________________ to determine whether such species or communities occur or are likely to occur on the site. Comply with the appropriate case or option below.

Case 1. Sites ___________________ Affected Species or Ecological Community
The prerequisite is satisfied if the consultation and any necessary biological surveys determine that no such imperiled species or ecological communities have been found or have a high likelihood of occurring.

OR
Case 2. Sites ________ Affected Species or Ecological Community
If the site has any affected species or ecological communities, meet either of the following two options.

OPTION 1. ______________________________________________
Comply with an approved habitat conservation plan under the U.S. ______________________ Species Act (or local equivalent for projects outside the U.S.) for each identified species or ecological community.

OR
OPTION 2. ______________________________________________________________
Work with a qualified _____________________ or ___________________, a conservation organization, or the appropriate national, state or local agency to create and implement a conservation plan that includes the following actions:
· Identify and map the extent of the habitat and the appropriate buffer, not less than __________, according to best available scientific information.
· If on-site protection can be accomplished, analyze threats from development and develop a ____________________ and management plan that eliminates or significantly reduces the threats.
· Protect the identified habitat and buffer in ______________________ by donating or selling the land or a conservation easement on the land to an accredited land trust, conservation organization, or relevant government agency.
· If any portion of the identified habitat and buffer cannot be protected in perpetuity, quantify the effects by acres (hectares) or number of plants and/or animals affected, and _______________ from development in perpetuity habitat of ___________________ or better quality, on-site or off-site, by donating or selling a conservation easement on it to an accredited land trust, conservation organization, or relevant government agency. The donation or easement must cover an amount of land __________ to or _________________ than the area that cannot be protected.

11. SSL Prerequisite Wetland and Water Body Conservation
Requirements
Limit development effects on _______________________, water bodies, and surrounding __________ land according to the requirements below.

Case 1. Sites without Sensitive Areas
Locate the project on a site that includes no __________________ wetlands, water bodies, land within ______________ of wetlands, and land within ______________ of water bodies.



Case 2. Sites with Sensitive Areas
If the site has __________________ wetlands, water bodies, land within __________________ of wetlands, or land within __________________ of water bodies, select one of the following two options:

OPTION 1. _________________________________________________________
Locate the project such that __________________ wetlands, water bodies, land within __________________ of wetlands, and land within __________________ of water bodies are not affected by ________ development, unless the development is ____________ improvements or is on ________________ developed land.

OR
OPTION 2. _________________________________________________________
Earn at least 1 point under GIB Credit Rainwater Management, and limit any development beyond ______________ improvements to __________ than the percentage of buffer land listed in Table 1.

Table 1. Maximum allowable area of development within buffer zone, by project density

	


Residential density
	



Nonresidential density
(FAR)*
	

Percentage of buffer land** where development beyond minor improvements is allowed

	DU/acre*
	DU/hectare*
	
	

	> 25
	> 62
	> 
	≤ 20%

	> 18 and ≤ 25
	> 45 and ≤ 62
	> 1.25 to ≤ 1.75
	≤ 15%

	> 10 and ≤ 18
	> 25 and ≤ 45
	> .75 to ≤ 1.25
	≤ 10%

	≤ 10
	≤ 25
	≤ .75
	≤ 5%


DU = dwelling unit; FAR = floor-area ratio.
* For this option, a mixed-use project may use ________________ its residential or its nonresidential density to determine the percentage of allowable development, regardless of which is higher.

** Buffer width may vary as long as the total buffer area is equal to the area within ________________ of wetlands and/or within ________________ of water bodies, minus excluded features (see list of minor improvements, below). In no case may the buffer width be less than ________________ for wetlands and ________________ for water bodies, measured from the edge. Inside this minimum buffer, only minor improvements and/or improvements that result in no ecological impairment of the wetland or water body, as determined by a qualified ______________________, are allowed.

For All Projects
Comply with all local, state, and national regulations pertaining to wetland and water body conservation.
The following features are not considered wetlands, water bodies, or buffer land that must be protected for the purposes of this prerequisite:
_______________________ developed land;
_______________________ water bodies (such as industrial mining pits, concrete-lined canals, or stormwater retention ponds) that lack natural edges and floors or native ecological communities in the water and along the edge;
_______________________ linear wetlands that result from the interruption of natural drainages by existing rights-of-way; and
_______________________ that were man-made incidentally and have been rated “poor” for all measured wetland functions, as assessed by a qualified biologist using a method that is accepted by state or regional permitting agencies (or a local equivalent for projects outside the U.S.).
Minor improvements within the buffer may be undertaken to enhance appreciation for the wetland or water body, provided such facilities are open to _________________ access. Only the following improvements are permitted:
__________________ and pedestrian pathways no more than _____________ wide, of which no more than ________ total feet may be _________________________ ;
activities to maintain or restore __________________ natural communities and/or natural hydrology;
one single-story ________________________ not exceeding 500 square feet per 300 linear feet of buffer, on average;
_________________ changes necessary to ensure public access;
_________________, limited to one per __________ linear feet of buffer, on average, not exceeding 500 square feet each, for tables, benches, and access for nonmotorized recreational watercraft;
removal of _______________________________ trees (up to 75% of dead trees), trees smaller than ________ inches in diameter at breast height, trees with a condition rating of less than __________, as based on an assessment by an _______________________ certified by the International Society of Arboriculture (ISA) using ISA standard measures or for projects outside the U.S.an equivalent certified professional utilizing equivalent methodology; and
______________________ remediation activities.

Off-street _________________________ is not considered a minor improvement.

Direct development of wetlands and water bodies is prohibited, except for minimal-impact structures, such as an elevated boardwalk, that allow ______________ to the water for educational and recreational purposes. Structures that protrude into wetlands or water bodies may be replaced, provided the replacement structure has the same or smaller footprint and a similar height.

The U.S. loses about __________________ acres (_______________ hectares) of wetlands each year.

12. SSL Prerequisite Agricultural Land Conservation
Requirements
Locate the project on a site that is not within a state or locally designated agricultural preservation district (or local equivalent for projects outside the U.S.), unless any changes made to the site conform to the requirements for development within the district (as used in this requirement, “district” does not equate to land-use zoning).

Meet the requirements of one of the following five options.
OPTION 1. _____________________ Sites
Locate the project on an __________________ site.

OR
OPTION 2. Sites Served by __________________
Comply with SLL Prerequisite Smart Location, Option 3, ________________________________.

OR
OPTION 3. Development Rights ___________________________ Area
Locate the project within a designated receiving area for development rights under a publicly administered __________________________ protection program that provides for the transfer of development rights from lands designated for conservation to lands designated for development.

OR
OPTION 4. Sites Without Affected _____________________
Locate the project’s development footprint such that it does not disturb ________________ farmland, ________________ farmland, or farmland of statewide or local importance as defined by the U.S. Code of Federal Regulations, Title 7, Volume 6,Parts 400 to 699, Section 657.5 and identified in a state Natural Resources Conservation Service soil survey (or local equivalent for projects outside the U.S.).

OR
OPTION 5. Sites With Affected ________________ 
If development footprint affects land with prime farmland, unique farmland, or farmland of statewide or local importance as defined by the U.S. Code of Federal Regulations, Title 7, Volume 6, Parts 400 to 699, Section 657.5 and identified in a state Natural Resources Conservation Service soil survey (or local equivalent for projects outside the U.S.), ________________ the loss through the purchase or donation of easements providing __________________________ protection from development on land with comparable soils in accordance with the ratios based on densities per acre (per hectare) of buildable land listed in Tables 1 and 2.

Table 1. Mitigation ratios for projects in large metropolitan or micropolitan statistical areas (pop. 250,000 or more)
	Residential density
	
Nonresidential density (FAR of buildable land available for nonresidential use)
	
Mitigation ratio (area of easement : area
of project on prime, unique, or significant farmland)

	DU per acre of
buildable land available for residential use
	DU per hectare of
buildable land available for residential use
	
	

	> 7 and ≤ 8.5
	> 17.5 and ≤ 21
	> 0.50 and ≤ 0.67
	2 to 1

	> 8.5 and ≤ 10
	> 21 and ≤ 25
	> 0.67 and ≤ 0.75
	1.5 to 1

	> 10 and ≤ 11.5
	> 25 and ≤ 28.5
	> 0.75 and ≤ 0.87
	1 to 1

	> 11.5 and ≤ 13
	> 28.5 and ≤ 32
	> 0.87 and ≤ 1.0
	.5 to 1

	> 13
	> 32
	> 1.0
	No mitigation



Table 2. Mitigation ratios for projects in small metropolitan or micropolitan statistical areas (pop. less than 250,000)
	Residential density
	Nonresidential density
(FAR of buildable land available for nonresidential use)
	Mitigation ratio (area
of easement : area of project on prime, unique, or significant farmland)

	DU/acre of buildable
land available for residential use
	DU/hectare of
buildable land available for residential use
	
	

	> 7 and ≤ 8
	> 17.5 and ≤ 20
	> 0.50 and ≤ 0.58
	2 to 1

	> 8 and ≤ 9
	> 20 and ≤ 22
	> 0.58 and ≤ 0.67
	1 to 1

	> 9 and ≤ 10
	> 22 and ≤ 25
	> 0.67 and ≤ 0.75
	0.5 to 1

	> 10
	> 25
	> 0.75
	No mitigation


DU = dwelling unit; FAR = floor-area ratio.

All off-site mitigation must be located within ____________________ of the project.

Up to ___________ of the affected farmland area may be subtracted from the mitigation area required of the project in Tables 1 and 2 if it is permanently dedicated for community _________________. Portions of parking structures devoted ____________________________ to parking must be excluded from the numerator when calculating the floor-area ratio (FAR).

The mitigation _________________ for a mixed-use project is calculated as follows:
1. Determine the total floor area of all residential and nonresidential uses.
2. Calculate the percentage residential and percentage nonresidential of the total floor area.
3. Determine the density of the residential and nonresidential components as measured in ______________________________________ and ____________ respectively.
4. Referring to Tables 1 and 2, find the appropriate mitigation ratios for the residential and nonresidential components.
5. If the mitigation ratios are different, multiply the mitigation ratio of the residential component by its percentage of the total floor area, and multiply the mitigation ratio of the nonresidential component by its percentage.
6. Add the two numbers produced by step 5. The result is the mitigation ratio.

13. SSL Prerequisite Floodplain Avoidance
Requirements
Case 1. Sites without Flood Hazard Areas
Locate on a site that is __________________ outside any flood hazard area shown on a legally adopted flood hazard map or otherwise legally designated by the local jurisdiction or the state. For projects in places without legally adopted flood hazard maps or legal designations, locate on a site that is entirely outside any floodplain subject to a ________ or greater chance of flooding in any given year.

Case 2. Infill or Previously Developed Sites with Flood Hazard Areas
Locate the project on an ____________ site or a ____________________ developed site and select one of the following two options.

Option 1. American Society of Civil Engineers Standard
For any portion of the site within the flood hazard area, design buildings in accordance with American Society of Civil Engineers Standard _____________ (ASCE 24).

If the project includes construction of a critical facility that is intended to remain operational in the event of a flood, or whose function is critical for postflood recovery, design the facility to be protected and operable at the floodwater levels specified in ASCE 24, or at the water levels represented by a __________ annual chance (________ year) flood, whichever is higher. For the purpose of this requirement, critical facilities include, but are not limited to, _________________, emergency operations centers, building or portions of buildings designated as emergency shelters, water and _____________________ treatment facilities, and ___________ and _______________ stations.

OR

Option 2. National Flood Insurance Program
For any portion of the site within the flood hazard area, design buildings in accordance with _______________________________________________________________ (NFIP) requirements. Project outside the U.S. may use a local equivalent to NFIP if the program is equal to or more stringent than NFIP and is administered at the national level.

If the project includes construction of a critical facility that is intended to remain operational in the event of a flood, or whose function is critical for postflood recovery, design the facility to be protected and operable at the floodwater levels specified in ASCE 24, or at the water levels represented by a __________ annual chance (________ year) flood, whichever is higher. For the purpose of this requirement, critical facilities include, but are not limited to, _________________, emergency operations centers, building or portions of buildings designated as emergency shelters, water and _____________________ treatment facilities, and ___________ and _______________ stations.




Case 3. All Other Sites with Flood Hazard Areas
Meet the requirements of one of the following two options.
 
Option 1. American Society of Civil Engineers Standard
Previously developed portions of the site
On portions of the site that are previously developed and in the flood hazard area, design buildings in accordance with American Society of Civil Engineers Standard _____________ (ASCE 24).

Nonpreviously developed portions of the site
On portions of the site that are not previously developed and in the flood hazard area, do not develop on land that is within either a regulatory ____________________ or a coastal high hazard area (Zone _____), as shown on the flood hazard map.

On all other portions of the site that are not previously developed and in the flood hazard area, design buildings in accordance with _____________.

Critical facilities in the flood hazard area
If the project involves a critical facility that is intended to remain operational in the event of a flood, or whose function is critical for postflood recovery, design the facility to be protected and operable at the floodwater levels specified in __________________ or at the water levels represented by a 0.2% annual chance (500-year) flood, whichever is higher. For the purpose of this requirement, critical facilities include, but are not limited to, hospitals, emergency operations centers, building or portions of buildings designated as emergency shelters, water and sewage treatment facilities, and fire and police stations.

OR

Option 2. National Flood Insurance Program
Previously developed portions of the site
On portions of the site that are previously developed and in the flood hazard area, design buildings in accordance with National Flood Insurance Program (NFIP) requirements. Project outside of the U.S. may use a local equivalent to NFIP if the program is equal to or more stringent than NFIP and is administered at the national level.

Nonpreviously developed portions of the site
On portions of the site that are not previously developed and in the flood hazard area, do not develop on land that is within either a regulatory ____________________ or a coastal high hazard area (Zone _____), as shown on the flood hazard map.

On all other portions of the site that are not previously developed and in the flood hazard area, design buildings in accordance with ____________.

Critical facilities in the flood hazard area
If the project involves a critical facility that is intended to remain operational in the event of a flood, or whose function is critical for postflood recovery, design the facility to be protected and operable at the water levels represented by a 0.2% annual chance (500-year) flood. For the purpose of this requirement, critical facilities include, but are not limited to, hospitals, emergency operations centers, building or portions of buildings designated as emergency shelters, water and sewage treatment facilities, and fire and police stations.




14. SSL Credit Preferred Locations
Requirements
Achieve any combination of requirements in the following three options, for a total of up to 10 points.

OPTION 1. LOCATION TYPE (1–5 POINTS)
Locate the project in one of the following locations:
a _________________ developed site that is not an _________________ site or __________ site (1 point);
an _________________ site that is also a _________________ developed site (2 points);
an __________ site that is not a _________________ developed site (3 points); or
an __________ site that is also a _________________ developed site (5 points).

AND/OR
OPTION 2. ______________________________________  (1-5 POINTS)
Locate the project in an area that has existing connectivity, as listed in Table 1. Measure connectivity one of two ways:
within ___________________ of the project boundary; or
within the project and within ___________________ of the project boundary.
Intersections within the site cannot be counted if they were constructed or funded by the developer within the past ___________________.

Table 1. Points for connectivity

	Intersections
per square mile
	Intersections
per square kilometer
	Points

	200–249
	320–399
	1

	250–299
	400–479
	2

	300–349
	480–559
	3

	350–399
	560–639
	4

	> 400
	> 640
	5



AND/OR

OPTION 3. ________________________________________________________________ (3 POINTS)
Earn at least 2 points under NPD Credit Housing Types and Affordability, Option 2, Affordable Housing.
AND
Locate the project in one of the following high-priority redevelopment areas:
a site listed by the EPA National ________________________ List;
a Federal ________________________Zone site;
a Federal ________________________Community site;
a Federal ________________________Community site;
a Department of the Treasury Community Development Financial Institutions Fund ________________________ Low-Income Community (a subset of the New Markets Tax Credit Program);
a site in a U.S. Department of Housing and Urban Development’s ________________________Census Tract (QCT) or Difficult Development Area (DDA); or
a local ________________________ program administered at a national level for projects outside the U.S.

15. SSL Credit Brownfield Remediation
Requirements
OPTION 1. ___________________________________ (1 POINT)
At a project site identified as a brownfield or where __________ or _______________________ contamination has been identified, and the local, state, or national authority (whichever has jurisdiction) requires its remediation, perform remediation to the satisfaction of that authority.
OR
OPTION 2. ____________________________________________________ (2 POINTS)
Achieve the requirements in Option 1.

AND
Locate the project in one of the following high-priority redevelopment areas:
a site listed by the EPA National ________________________ List;
a Federal ________________________Zone site;
a Federal ________________________Community site;
a Federal ________________________Community site;
a Department of the Treasury Community Development Financial Institutions Fund ________________________ Low-Income Community (a subset of the New Markets Tax Credit Program);
a site in a U.S. Department of Housing and Urban Development’s ________________________Census Tract (QCT) or Difficult Development Area (DDA); or
a local ________________________ program administered at a national level for projects outside the U.S.

16. SSL Credit Access to Quality Transit
Requirements
Locate the project on a site with existing or planned transit service (i.e., service with the funding commitments as specified in SLL Prerequisite Smart Location) such that at least _________ of dwelling units and nonresidential use entrances (inclusive of existing buildings) are within a ___________ walking distance of at least ________ bus or streetcar stop, or within a ___________ walking distance of at least _______ bus rapid transit stop, light or heavy rail station, commuter rail station, or commuter ferry terminal. The transit service at the stop(s) in aggregate must meet the minimums listed in Tables 1 and 2.

Projects must meet the requirements for ___________ weekday and weekend trips and provide service ______________ day.

Table 1. Minimum daily transit service for projects with multiple transit types (bus, streetcar, rail, or ferry).

	Weekday trips
	Weekend trips
	Points

	60
	40
	1

	76
	50
	2

	100
	65
	3

	132
	85
	4

	180
	130
	5

	246
	150
	6

	320
	200
	7



Table 2. Minimum daily transit service for projects with commuter rail or ferry service only

	Weekday trips
	Weekend trips
	Points

	24
	6
	1

	40
	8
	2

	60
	12
	3




Projects served by two or more transit routes such that no one route provides more than ________ of the prescribed levels may earn an additional point, up to the maximum number of points.

If existing transit service is temporarily rerouted outside the required distances for less than _______ years, the project may meet the requirements, provided the local transit agency has committed to restoring the routes with service at or above the prior level.

17. SSL Credit Bicycle Facilities
Requirements
Meet the following requirements in ___________ of all new buildings. The buildings that do not have bicycle storage may not exceed __________ of the total project building floor area.

Non-Residential (excluding Retail) Buildings
Provide ________________________ bicycle storage for at least ________ of peak visitors, but no fewer than ____________ storage spaces per building.

Provide ________________________ bicycle storage for at least ________ of all regular building occupants, but no fewer than ________ storage spaces per building in addition to the short-term bicycle storage spaces. Provide at least ________ on-site shower with changing facility for the first ________ regular building occupants and one additional shower for every ________ regular building occupants thereafter.

Multi-unit Residential Buildings
Provide ________________________ bicycle storage for at least __________ of all peak visitors, but no fewer than ________ storage spaces per building.

Provide ________________________ bicycle storage for at least __________ of all regular building occupants, but no less than __________ storage space per residential __________.

Retail Buildings
Provide at least __________ short-term bicycle storage spaces for every ________________ square feet, but no fewer than __________ storage spaces per building.

Provide long-term bicycle storage for at least __________ regular building occupants, but no fewer than __________ storage spaces per building in addition to the short-term bicycle storage.

Provide at least one on-site _______________ with changing facility for the first _________ regular building occupants and one additional shower for every ____________ regular building occupants thereafter.

Mixed-Use Buildings
Meet the above requirements for the project’s non-residential, multi-unit residential, and retail spaces.

For all projects:
Short-term bicycle storage must be within ____________ feet walking distance of any ____________ entrance. Long- term bicycle storage must be within ____________ feet walking distance of any __________________ entry. It must be easily accessible to all building users.

Shower and changing facility requirements may be met by providing the equivalent of free access to on-site health club shower facilities, if the health club can be accessed ___________________ going outside.
 
Additionally, meet the requirements of at least one of the following two options.

Option 1. Bikable Location (1 point)
Locate the project such that the project boundary is within ______________ bicycling distance of an existing bicycle ______________________ that connects to at least one of the following.
at least __________ diverse uses (see Appendix 1);
a _________________ or employment center, if the project total floor area is _______ or more residential; or a bus rapid transit stop, light or heavy rail station, commuter rail station, or ferry terminal. All destinations must be within a ________________________ bicycling distance of the project boundary.

AND/OR

Option 2. Bicycle Network (1 point)
Design the project such that at least 50% of _______________________________ and nonresidential use entrances are located on an existing or planned bicycle network extending at least __________ continuous miles. Within those 3 miles, the network must connect to one of the following:
a ___________________;
an ______________________________ center; or
at least __________diverse uses (see Appendix 1).

18. SSL Credit Housing and Jobs Proximity
Requirements
Option 1. Project with Affordable Residential Component (3 points)
Include a residential component equaling at least ___________ of the project’s total building floor area (exclusive of ___________________ structures), and locate or design the project such that its geographic center (or boundary if the project exceeds 500 acres [200 hectares]) is within a _________________ walking distance of existing full-time equivalent jobs whose number equals or exceeds the number of dwelling units in the project. Satisfy the requirements necessary to earn at least 1 point under NPD Credit Housing Types and Affordability, Option 2, Affordable Housing.

Option 2. Project with Residential Component (2 points)
Include a residential component equaling at least ____________ of the project’s total building floor area (exclusive of parking structures) and locate or design the project such that its geographic center (or boundary if the project exceeds 500 acres [200 hectares]) is within a ______________ walking distance of existing full-time equivalent jobs whose number equals or exceeds the number of dwelling units in the project.

Option 3. Infill Project with Nonresidential Component (1 point)
Include a nonresidential component equaling at least ____________ of the project’s total building floor area (exclusive of parking structures) and locate on an ________________ site whose geographic center (or boundary if the project exceeds 500 acres [200 hectares]) is within a __________________ walking distance of an existing rail transit, ferry, or tram stop and within a __________________ walking distance of existing dwelling units whose number equals or exceeds ____________ of the number of new full-time equivalent jobs located in the project.

19. SSL Credit Steep Slope Protection
Requirements
The following requirements apply to projects sites that have slopes greater than ________.

Ensure that the share of the development footprint on existing slopes __________________ than 15% is greater than the share of the project site with existing slopes greater than 15%.

On any existing, previously developed slopes steeper than 15%, restore the slope area with _______________________ or __________________ plants, according to Table 1. In addition, on any existing, undeveloped slopes steeper than 15%, limit the development area according to Table 1.




Table 1. Required restoration and protection areas of slope

	Slope
	Previously developed slopes:
% of area to be restored
	Undeveloped slopes:
% of area permitted for development

	> 40%
	100%
	No development permitted

	26% to 40%
	60%
	40%

	>15% to 25%
	40%
	60%



For undeveloped slopes steeper than ____________, do not disturb portions of the project site within __________________ horizontally of the top of the slope and __________________ horizontally from the toe of the slope.

Develop _________________________, ______________________, and _____________________ (CC&Rs), development agreements, or other binding documents that will protect all steep slopes in perpetuity.

20. SSL Credit Site Design for Habitat or Wetland and Water Body Conservation
Requirements
Case 1. Sites without Significant Habitat or Wetlands and Water Bodies (1 point)
Locate the project on a site that does not have significant ___________________, as defined in Case 2 of this credit, and is not within ___________________ of such habitat. Fulfill the requirements of Option 1 or 2(a) under SLL Prerequisite Wetland and Water Body Conservation.

Case 2. Sites with Habitat or Wetlands or Water Bodies (1 point)
Meet the requirements of Option 1 or Option 2.

Option 1. Sites with Significant Habitat
Work with both the state’s Natural Heritage Program and the state fish and wildlife agency (or local equivalent agency for projects outside the U.S.) to delineate identified significant habitat on the site. Do not disturb significant _____________________ or portions of the site within an appropriate ______________ around the habitat. The geographic extent of the habitat and buffer must be identified by a qualified ________________________, a nongovernmental conservation organization, or the appropriate state, regional, or local agency. Protect significant habitat and its identified buffers from development by donating or selling the land, or a conservation easement on the land, to an accredited land trust, conservation organization, or relevant government agency (a deed covenant is not sufficient to meet this requirement) for the purpose of long-term conservation.

Identify and commit to ongoing management activities, along with parties responsible for management and funding available, such that habitat is maintained in ______________________ condition or better for a minimum of _____________ years after the project is built out. The requirement for identifying ongoing management activities may also be met by earning SLL Credit Long-Term Conservation Management of Habitat or Wetlands and Water Bodies.

Significant habitat for this credit is as follows:

Endangered species acts. Habitat for species that are listed or are candidates for listing under state or national endangered species acts, habitat for species of special concern in the state, and habitat for species or ecological communities classified as ________________________________________________________ (local equivalent standards for threatened and endangered species may be used in countries outside the U.S. that do not have access to NatureServe data);
Locally or regionally ______________________ habitat. Locally or regionally significant habitat of any size, or patches of predominantly native vegetation at least 150 acres (60 hectares) (even if part of the area lies outside the project boundary); and
Habitat flagged for ________________________. Habitat flagged for conservation under a regional or state conservation or green infrastructure plan.

OR

Option 2. Sites with Wetlands and Water Bodies (1 point)
Design the project to conserve ____________ of all water bodies, wetlands, land within ____________ of water bodies, and land within ____________ of wetlands on the site. Using a qualified biologist, conduct an assessment, or compile existing assessments, showing the extent to which those water bodies or wetlands provide (1) water _________________ maintenance; (2) wildlife habitat; and (3) _________________ function maintenance, including flood protection. Assign appropriate _________________, measuring not less than _________________ for water bodies and _________________ for wetlands, based on the functions provided, contiguous soils and slopes, and contiguous land uses. Do not disturb wetlands, water bodies, or their buffers, and protect them from development by donating or selling the land, or a conservation easement on the land, to an accredited land trust, conservation organization, or relevant government agency (a deed covenant is not sufficient to meet this requirement) for the purpose of long-term conservation.

Identify and commit to ongoing management activities, along with parties responsible for management and funding available, such that habitat is maintained in preproject condition or better for a minimum of ____________ years after the project is built out. The requirement for identifying ongoing management activities may also be met by earning SLL Credit Long-Term Conservation Management of Habitat or Wetlands and Water Bodies. The project does not meet the requirements if it degrades habitat for species identified in endangered species acts or habitat flagged for conservation in Option 1.

For All Projects
The following features are not considered wetlands, water bodies, or buffer land that must be protected:
__________________________ developed land;
man-made __________________________ (such as industrial mining pits, concrete-lined canals, or __________________________ retention ponds) that lack natural edges and floors or native ecological communities in the water and along the edge;
man-made linear __________________________ that result from the interruption of natural drainages by existing rights-of-way; and
wetlands that were created incidentally by __________________ activity and have been rated ―poor for all measured wetland functions, as assessed by a qualified biologist using a method that is accepted by state or regional permitting agencies (or a local equivalent method for projects outside the U.S.).

21. SSL Credit Restoration of Habitat or Wetlands and Water Bodies
Requirements
Using only ________________ plants, restore predevelopment native ecological communities, water bodies, or wetlands on the project site in an area equal to or greater than ________ of the development footprint.

Work with a qualified _______________________ to ensure that restored areas will have the native species assemblages, hydrology, and other habitat characteristics that likely occurred in predevelopment conditions. 

Protect such areas from development by _______________________ or selling the land, or a conservation easement on the land, to an accredited land trust, conservation organization or relevant government agency (a deed covenant is not sufficient to meet this requirement) for the purpose of long-term conservation.
Identify and commit to __________________ management activities, along with parties responsible for management and funding available, so that restored areas are maintained for a minimum of ________ years after the project is built out or the restoration is completed, whichever is later. The requirement for identifying ongoing management activities may also be met by earning SLL Credit Long-Term Conservation Management of Habitat or Wetlands and Water Bodies.

The project does not meet the requirements if it has negative effects on habitat for species identified in endangered species acts or habitat flagged for conservation in Option 1 of SLL Credit Site Design for Habitat or Wetland and Water Body Conservation.

22. SSL Credit Long-Term Conservation Management of Habitat or Wetlands and Water Bodies
Requirements
Create and commit to implementing a long-term (at least _____-year) management plan for existing or recently restored on-site __________________________, __________________________, or __________________________ and their __________________________, and create a guaranteed funding source for management.

Involve a qualified __________________________or a professional from a natural resources agency or natural resources consulting firm in writing the management plan and conducting or evaluating the ongoing management.

The plan must include biological objectives consistent with habitat or water resource conservation, and it must identify the following:
procedures and personnel for __________________________the conservation areas;
__________________________ implementation costs and funding sources; and
any _________________ that the project poses for habitat or water resources within conservation areas (e.g., introduction of exotic species, intrusion of residents in habitat areas) and measures to substantially reduce those threats.

The project does not meet the requirements if it has negative effects on habitat for species identified in endangered species acts or habitat flagged for conservation in Option 1 of SLL Credit Site Design for Habitat or Wetland and Water Body Conservation.
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